Pre-Insulated curved pipes – Construction Site / Facility

Pre-insulated curved pipes must be bent from the inside using mobile technology directly on the construction site, at the on-site pipe storage area, or at the facility, without any thermal influence.
The required bending angle must be precisely tailored to the specific installation situation and must not exceed a deviation of ±0.2°.

The radii and straight sections of the curved pipes for the supply and return lines must be manufactured individually so that they follow the route of the pipeline as closely as possible.
