Pre-Insulated curved pipes - Facility made

Pre-Insulated curved pipes must be bent at the facility using mobile technology, without thermal influence, and from the inside.
The required bending angle must be precisely tailored to the specific installation situation and must not exceed a deviation of ±0.2°.

The radii and straight sections of the curved pipes for the supply and return lines must be manufactured individually so that they follow the route of the pipeline as closely as possible.

